**LUMBER**

TWO 8 FOOT LONG 2 X 4

TWO 8 FOOT LONG 2 X 2

ONE 8 FOOT LONG 2 X 8

ONE 1 INCH DIAMETER WOOD DOWEL AT LEAST 36 INCHES LONG

ONE SHEET 4 FOOT X 8 FOOT ¾ INCH PLYWOOD

THIN WOOD FOR CRATE SLATS

**HARDWARE:**

2 EA ½”-13 X 36” THREADED STEEL ROD (AXLES)

2 EA 7/32 X 6 ¼” TURNBUCKLE (AXLES)

2 EA ¼” X 5” EYEBOLT WITH NUT (AXLES)

2 EA 1/8” QUICK LINK (AXLES)

1 PK ¼” WASHERS (AXLES)

8 EA ½” X 3” MENDING PLATE WITH SCREWS (AXLES)

3 EA ¾” AWNING PULLEY (STEERING AND BRAKES)

1 PK #14 X 1 ¾” WOOD SCREWS (STEERING PULLEYS)

1 EA 1” X ¾” PVC REDUCER BUSHING (STEERING)

1 PKG 1/16” X 2” COTTER PINS (STEERING)

15 FT 1/16”-1/8” WIRE ROPE (STEERING AND BRAKES)

4 EA WIRE ROPE CLAMP (STEERING AND BRAKES)

1 EA 3/16” X 5” TURNBUCKLE (BRAKES)

1 EA 1/8” QUICK LINK (BRAKES)

6 EA 3” BUTT HINGES WITH SCREWS (BRAKES)

4 EA ¼” X 3” EYEBOLT WITH NUT (BRAKES)

2 EA ¼” X 1 ½ SCREW IN EYEBOLT (BRAKES)

1 EA 5/8” X 6 ½” SPRING (BRAKES)

1 EA ½” X 5” HEX HEAD BOLT (FRONT AXLE)

2 EA ½” X 4” HEX HEAD BOLT (REAR AXLE)

16 EA ½” WASHER (WHEELS AND AXLES)

7 EA ½” X 13 LOCKNUT (WHEELS AND AXLES)

6 EA ¼” X 3” LAG BOLTS (FRAME)

1 BOX #10 X 3” WOOD SCREWS

1 BOX #8 X 1 ¼” WOOD SCREWS

1 PKG #8 X 2 ½” WOOD SCREWS

1 PKG #8 X 2” WOOD SCREWS

1 16 OZ BOTTLE OF TITEBOND III WOOD GLUE